# This file is a general .ucf for Nexys2 rev A board
# To use it in a project:
# - remove or comment the lines corresponding to unused pins
# - rename the used signals according to the project


## clock pin for Nexys 2 Board
NET "clk"   LOC = "B8"; # Bank = 0, Pin name = IP_L13P_0/GCLK8, Type = GCLK, Sch name = GCLK0
##NET "clk1" LOC = "U9"; # Bank = 2, Pin name = IO_L13P_2/D4/GCLK14, Type = DUAL/GCLK, Sch name = GCLK1
#
## Leds
NET "Led<0>"  LOC = "J14"; # Bank = 1, Pin name = IO_L14N_1/A3/RHCLK7, Type = RHCLK/DUAL, Sch name = JD10/LD0
NET "Led<1>"  LOC = "J15"; # Bank = 1, Pin name = IO_L14P_1/A4/RHCLK6, Type = RHCLK/DUAL, Sch name = JD9/LD1
NET "Led<2>"  LOC = "K15"; # Bank = 1, Pin name = IO_L12P_1/A8/RHCLK2, Type = RHCLK/DUAL, Sch name = JD8/LD2
NET "Led<3>"  LOC = "K14"; # Bank = 1, Pin name = IO_L12N_1/A7/RHCLK3/TRDY1, Type = RHCLK/DUAL, Sch name = JD7/LD3
#NET "Led<4>"  LOC = "E17"; # Bank = 1, Pin name = IO, Type = I/O, Sch name = LD4
#NET "Led<5>"  LOC = "P15"; # Bank = 1, Pin name = IO, Type = I/O, Sch name = LD5
#NET "Led<6>"  LOC = "F4";  # Bank = 3, Pin name = IO, Type = I/O, Sch name = LD6
#NET "Led<7>"  LOC = "R4";  # Bank = 3, Pin name = IO/VREF_3, Type = VREF, Sch name = LD7
 
## Switches
#NET "sw<0>" LOC = "G18"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW0
#NET "sw<1>" LOC = "H18"; # Bank = 1, Pin name = IP/VREF_1, Type = VREF, Sch name = SW1
#NET "sw<2>" LOC = "K18"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW2
#NET "sw<3>" LOC = "K17"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW3
#NET "sw<4>" LOC = "L14"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW4
#NET "sw<5>" LOC = "L13"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW5
#NET "sw<6>" LOC = "N17"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW6
#NET "sw<7>" LOC = "R17"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = SW7
 
## Buttons
#NET "btn<0>" LOC = "B18"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = BTN0
#NET "btn<1>" LOC = "D18"; # Bank = 1, Pin name = IP/VREF_1, Type = VREF, Sch name = BTN1
#NET "btn<2>" LOC = "E18"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = BTN2
#NET "btn<3>" LOC = "H13"; # Bank = 1, Pin name = IP, Type = INPUT, Sch name = BTN3
 
## 7 segment display
#NET "seg<0>" LOC = "L18"; # Bank = 1, Pin name = IO_L10P_1, Type = I/O, Sch name = CA
#NET "seg<1>" LOC = "F18"; # Bank = 1, Pin name = IO_L19P_1, Type = I/O, Sch name = CB
#NET "seg<2>" LOC = "D17"; # Bank = 1, Pin name = IO_L23P_1/HDC, Type = DUAL, Sch name = CC
#NET "seg<3>" LOC = "D16"; # Bank = 1, Pin name = IO_L23N_1/LDC0, Type = DUAL, Sch name = CD
#NET "seg<4>" LOC = "G14"; # Bank = 1, Pin name = IO_L20P_1, Type = I/O, Sch name = CE
#NET "seg<5>" LOC = "J17"; # Bank = 1, Pin name = IO_L13P_1/A6/RHCLK4/IRDY1, Type = RHCLK/DUAL, Sch name = CF
#NET "seg<6>" LOC = "H14"; # Bank = 1, Pin name = IO_L17P_1, Type = I/O, Sch name = CG
#NET "dp"     LOC = "C17"; # Bank = 1, Pin name = IO_L24N_1/LDC2, Type = DUAL, Sch name = DP
 
#NET "an<0>" LOC = "F17"; # Bank = 1, Pin name = IO_L19N_1, Type = I/O, Sch name = AN0
#NET "an<1>" LOC = "H17"; # Bank = 1, Pin name = IO_L16N_1/A0, Type = DUAL, Sch name = AN1
#NET "an<2>" LOC = "C18"; # Bank = 1, Pin name = IO_L24P_1/LDC1, Type = DUAL, Sch name = AN2
#NET "an<3>" LOC = "F15"; # Bank = 1, Pin name = IO_L21P_1, Type = I/O, Sch name = AN3
 
## VGA Connector 
#NET "vgaRed<1>"   LOC = "R9"; # Bank = 2, Pin name = IO/D5, Type = DUAL, Sch name = RED0
#NET "vgaRed<2>"   LOC = "T8"; # Bank = 2, Pin name = IO_L10N_2, Type = I/O, Sch name = RED1
#NET "vgaRed<3>"   LOC = "R8"; # Bank = 2, Pin name = IO_L10P_2, Type = I/O, Sch name = RED2
#NET "vgaGreen<1>" LOC = "N8"; # Bank = 2, Pin name = IO_L09N_2, Type = I/O, Sch name = GRN0
#NET "vgaGreen<2>" LOC = "P8"; # Bank = 2, Pin name = IO_L09P_2, Type = I/O, Sch name = GRN1
#NET "vgaGreen<3>" LOC = "P6"; # Bank = 2, Pin name = IO_L05N_2, Type = I/O, Sch name = GRN2
#NET "vgaBlue<2>"  LOC = "U5"; # Bank = 2, Pin name = IO/VREF_2, Type = VREF, Sch name = BLU1
#NET "vgaBlue<3>"  LOC = "U4"; # Bank = 2, Pin name = IO_L03P_2/DOUT/BUSY, Type = DUAL, Sch name = BLU2
 
#NET "Hsync" LOC = "T4"; # Bank = 2, Pin name = IO_L03N_2/MOSI/CSI_B, Type = DUAL, Sch name = HSYNC
#NET "Vsync" LOC = "U3"; # Bank = 2, Pin name = IO_L01P_2/CSO_B, Type = DUAL, Sch name = VSYNC
 
## RS232 connector
#NET "RsRx" LOC = "U6"; # Bank = 2, Pin name = IP, Type = INPUT, Sch name = RS-RX
#NET "RsTx" LOC = "P9"; # Bank = 2, Pin name = IO, Type = I/O, Sch name = RS-TX
 
## PS/2 connector
#NET "PS2C" LOC = "R12"; # Bank = 2, Pin name = IO_L20N_2, Type = I/O, Sch name = PS2C
#NET "PS2D" LOC = "P11"; # Bank = 2, Pin name = IO_L18P_2, Type = I/O, Sch name = PS2D
 
## onBoard Cellular RAM and StrataFlash
#NET "MemOE"     LOC = "T2"; # Bank = 3, Pin name = IO_L24P_3, Type = I/O, Sch name = OE
#NET "MemWR"     LOC = "N7"; # Bank = 2, Pin name = IO_L07P_2, Type = I/O, Sch name = WE
 
#NET "RamAdv"    LOC = "J4"; # Bank = 3, Pin name = IO_L11N_3/LHCLK1, Type = LHCLK, Sch name = MT-ADV
#NET "RamCS"     LOC = "R6"; # Bank = 2, Pin name = IO_L05P_2, Type = I/O, Sch name = MT-CE
#NET "RamClk"    LOC = "H5"; # Bank = 3, Pin name = IO_L08N_3, Type = I/O, Sch name = MT-CLK
#NET "RamCRE"    LOC = "P7"; # Bank = 2, Pin name = IO_L07N_2, Type = I/O, Sch name = MT-CRE
#NET "RamLB"     LOC = "K5"; # Bank = 3, Pin name = IO_L14N_3/LHCLK7, Type = LHCLK, Sch name = MT-LB
#NET "RamUB"     LOC = "K4"; # Bank = 3, Pin name = IO_L13N_3/LHCLK5, Type = LHCLK, Sch name = MT-UB
#NET "RamWait"   LOC = "F5"; # Bank = 3, Pin name = IP, Type = INPUT, Sch name = MT-WAIT
 
#NET "FlashRp"    LOC = "T5"; # Bank = 2, Pin name = IO_L04N_2, Type = I/O, Sch name = RP#
#NET "FlashCS"    LOC = "R5"; # Bank = 2, Pin name = IO_L04P_2, Type = I/O, Sch name = ST-CE
#NET "FlashStSts" LOC = "D3"; # Bank = 3, Pin name = IP, Type = INPUT, Sch name = ST-STS
 
#NET "MemAdr<1>"  LOC = "J1"; # Bank = 3, Pin name = IO_L12P_3/LHCLK2, Type = LHCLK, Sch name = ADR1
#NET "MemAdr<2>"  LOC = "J2"; # Bank = 3, Pin name = IO_L12N_3/LHCLK3/IRDY2, Type = LHCLK, Sch name = ADR2
#NET "MemAdr<3>"  LOC = "H4"; # Bank = 3, Pin name = IO_L09P_3, Type = I/O, Sch name = ADR3
#NET "MemAdr<4>"  LOC = "H1"; # Bank = 3, Pin name = IO_L10N_3, Type = I/O, Sch name = ADR4
#NET "MemAdr<5>"  LOC = "H2"; # Bank = 3, Pin name = IO_L10P_3, Type = I/O, Sch name = ADR5
#NET "MemAdr<6>"  LOC = "J5"; # Bank = 3, Pin name = IO_L11P_3/LHCLK0, Type = LHCLK, Sch name = ADR6
#NET "MemAdr<7>"  LOC = "H3"; # Bank = 3, Pin name = IO_L09N_3, Type = I/O, Sch name = ADR7
#NET "MemAdr<8>"  LOC = "H6"; # Bank = 3, Pin name = IO_L08P_3, Type = I/O, Sch name = ADR8
#NET "MemAdr<9>"  LOC = "F1"; # Bank = 3, Pin name = IO_L05P_3, Type = I/O, Sch name = ADR9
#NET "MemAdr<10>" LOC = "G3"; # Bank = 3, Pin name = IO_L06P_3, Type = I/O, Sch name = ADR10
#NET "MemAdr<11>" LOC = "G6"; # Bank = 3, Pin name = IO_L07P_3, Type = I/O, Sch name = ADR11
#NET "MemAdr<12>" LOC = "G5"; # Bank = 3, Pin name = IO_L07N_3, Type = I/O, Sch name = ADR12
#NET "MemAdr<13>" LOC = "G4"; # Bank = 3, Pin name = IO_L06N_3/VREF_3, Type = VREF, Sch name = ADR13
#NET "MemAdr<14>" LOC = "F2"; # Bank = 3, Pin name = IO_L05N_3, Type = I/O, Sch name = ADR14
#NET "MemAdr<15>" LOC = "E1"; # Bank = 3, Pin name = IO_L03N_3, Type = I/O, Sch name = ADR15
#NET "MemAdr<16>" LOC = "M5"; # Bank = 3, Pin name = IO_L19P_3, Type = I/O, Sch name = ADR16
#NET "MemAdr<17>" LOC = "E2"; # Bank = 3, Pin name = IO_L03P_3, Type = I/O, Sch name = ADR17
#NET "MemAdr<18>" LOC = "C2"; # Bank = 3, Pin name = IO_L01N_3, Type = I/O, Sch name = ADR18
#NET "MemAdr<19>" LOC = "C1"; # Bank = 3, Pin name = IO_L01P_3, Type = I/O, Sch name = ADR19
#NET "MemAdr<20>" LOC = "D2"; # Bank = 3, Pin name = IO_L02N_3/VREF_3, Type = VREF, Sch name = ADR20
#NET "MemAdr<21>" LOC = "K3"; # Bank = 3, Pin name = IO_L13P_3/LHCLK4/TRDY2, Type = LHCLK, Sch name = ADR21
#NET "MemAdr<22>" LOC = "D1"; # Bank = 3, Pin name = IO_L02P_3, Type = I/O, Sch name = ADR22
#NET "MemAdr<23>" LOC = "K6"; # Bank = 3, Pin name = IO_L14P_3/LHCLK6, Type = LHCLK, Sch name = ADR23
 
#NET "MemDB<0>"  LOC = "L1"; # Bank = 3, Pin name = IO_L15P_3, Type = I/O, Sch name = DB0
#NET "MemDB<1>"  LOC = "L4"; # Bank = 3, Pin name = IO_L16N_3, Type = I/O, Sch name = DB1
#NET "MemDB<2>"  LOC = "L6"; # Bank = 3, Pin name = IO_L17P_3, Type = I/O, Sch name = DB2
#NET "MemDB<3>"  LOC = "M4"; # Bank = 3, Pin name = IO_L18P_3, Type = I/O, Sch name = DB3
#NET "MemDB<4>"  LOC = "N5"; # Bank = 3, Pin name = IO_L20N_3, Type = I/O, Sch name = DB4
#NET "MemDB<5>"  LOC = "P1"; # Bank = 3, Pin name = IO_L21N_3, Type = I/O, Sch name = DB5
#NET "MemDB<6>"  LOC = "P2"; # Bank = 3, Pin name = IO_L21P_3, Type = I/O, Sch name = DB6
#NET "MemDB<7>"  LOC = "R2"; # Bank = 3, Pin name = IO_L23N_3, Type = I/O, Sch name = DB7
#NET "MemDB<8>"  LOC = "L3"; # Bank = 3, Pin name = IO_L16P_3, Type = I/O, Sch name = DB8
#NET "MemDB<9>"  LOC = "L5"; # Bank = 3, Pin name = IO_L17N_3/VREF_3, Type = VREF, Sch name = DB9
#NET "MemDB<10>" LOC = "M3"; # Bank = 3, Pin name = IO_L18N_3, Type = I/O, Sch name = DB10
#NET "MemDB<11>" LOC = "M6"; # Bank = 3, Pin name = IO_L19N_3, Type = I/O, Sch name = DB11
#NET "MemDB<12>" LOC = "L2"; # Bank = 3, Pin name = IO_L15N_3, Type = I/O, Sch name = DB12
#NET "MemDB<13>" LOC = "N4"; # Bank = 3, Pin name = IO_L20P_3, Type = I/O, Sch name = DB13
#NET "MemDB<14>" LOC = "R3"; # Bank = 3, Pin name = IO_L23P_3, Type = I/O, Sch name = DB14
#NET "MemDB<15>" LOC = "T1"; # Bank = 3, Pin name = IO_L24N_3, Type = I/O, Sch name = DB15
 
## FX2 connector
#NET "PIO<0>"  LOC = "B4";  # Bank = 0, Pin name = IO_L24N_0, Type = I/O, Sch name = R-IO1
#NET "PIO<1>"  LOC = "A4";  # Bank = 0, Pin name = IO_L24P_0, Type = I/O, Sch name = R-IO2
#NET "PIO<2>"  LOC = "C3";  # Bank = 0, Pin name = IO_L25P_0, Type = I/O, Sch name = R-IO3
#NET "PIO<3>"  LOC = "C4";  # Bank = 0, Pin name = IO, Type = I/O, Sch name = R-IO4
#NET "PIO<4>"  LOC = "B6";  # Bank = 0, Pin name = IO_L20P_0, Type = I/O, Sch name = R-IO5
#NET "PIO<5>"  LOC = "D5";  # Bank = 0, Pin name = IO_L23N_0/VREF_0, Type = VREF, Sch name = R-IO6
#NET "PIO<6>"  LOC = "C5";  # Bank = 0, Pin name = IO_L23P_0, Type = I/O, Sch name = R-IO7
#NET "PIO<7>"  LOC = "F7";  # Bank = 0, Pin name = IO_L19P_0, Type = I/O, Sch name = R-IO8
#NET "PIO<8>"  LOC = "E7";  # Bank = 0, Pin name = IO_L19N_0/VREF_0, Type = VREF, Sch name = R-IO9
#NET "PIO<9>"  LOC = "A6";  # Bank = 0, Pin name = IO_L20N_0, Type = I/O, Sch name = R-IO10
#NET "PIO<10>" LOC = "C7";  # Bank = 0, Pin name = IO_L18P_0, Type = I/O, Sch name = R-IO11
#NET "PIO<11>" LOC = "F8";  # Bank = 0, Pin name = IO_L17N_0, Type = I/O, Sch name = R-IO12
#NET "PIO<12>" LOC = "D7";  # Bank = 0, Pin name = IO_L18N_0/VREF_0, Type = VREF, Sch name = R-IO13
#NET "PIO<13>" LOC = "E8";  # Bank = 0, Pin name = IO_L17P_0, Type = I/O, Sch name = R-IO14
#NET "PIO<14>" LOC = "E9";  # Bank = 0, Pin name = IO_L15P_0, Type = I/O, Sch name = R-IO15
#NET "PIO<15>" LOC = "C9";  # Bank = 0, Pin name = IO_L14P_0/GCLK10, Type = GCLK, Sch name = R-IO16
#NET "PIO<16>" LOC = "A8";  # Bank = 0, Pin name = IO, Type = I/O, Sch name = R-IO17
#NET "PIO<17>" LOC = "G9";  # Bank = 0, Pin name = IO, Type = I/O, Sch name = R-IO18
#NET "PIO<18>" LOC = "F9";  # Bank = 0, Pin name = IO_L15N_0, Type = I/O, Sch name = R-IO19
#NET "PIO<19>" LOC = "D10"; # Bank = 0, Pin name = IO_L11P_0/GCLK4, Type = GCLK, Sch name = R-IO20
#NET "PIO<20>" LOC = "A10"; # Bank = 0, Pin name = IO_L12N_0/GCLK7, Type = GCLK, Sch name = R-IO21
#NET "PIO<21>" LOC = "B10"; # Bank = 0, Pin name = IO_L12P_0/GCLK6, Type = GCLK, Sch name = R-IO22
#NET "PIO<22>" LOC = "A11"; # Bank = 0, Pin name = IO, Type = I/O, Sch name = R-IO23
#NET "PIO<23>" LOC = "D11"; # Bank = 0, Pin name = IO_L09N_0, Type = I/O, Sch name = R-IO24
#NET "PIO<24>" LOC = "E10"; # Bank = 0, Pin name = IO_L11N_0/GCLK5, Type = GCLK, Sch name = R-IO25
#NET "PIO<25>" LOC = "B11"; # Bank = 0, Pin name = IO/VREF_0, Type = VREF, Sch name = R-IO26
#NET "PIO<26>" LOC = "C11"; # Bank = 0, Pin name = IO_L09P_0, Type = I/O, Sch name = R-IO27
#NET "PIO<27>" LOC = "E11"; # Bank = 0, Pin name = IO_L08P_0, Type = I/O, Sch name = R-IO28
#NET "PIO<28>" LOC = "F11"; # Bank = 0, Pin name = IO_L08N_0, Type = I/O, Sch name = R-IO29
#NET "PIO<29>" LOC = "E12"; # Bank = 0, Pin name = IO_L06N_0, Type = I/O, Sch name = R-IO30
#NET "PIO<30>" LOC = "F12"; # Bank = 0, Pin name = IO_L06P_0, Type = I/O, Sch name = R-IO31
#NET "PIO<31>" LOC = "A13"; # Bank = 0, Pin name = IO_L05P_0, Type = I/O, Sch name = R-IO32
#NET "PIO<32>" LOC = "B13"; # Bank = 0, Pin name = IO_L05N_0/VREF_0, Type = VREF, Sch name = R-IO33
#NET "PIO<33>" LOC = "E13"; # Bank = 0, Pin name = IO, Type = I/O, Sch name = R-IO34
#NET "PIO<34>" LOC = "A14"; # Bank = 0, Pin name = IO_L04N_0, Type = I/O, Sch name = R-IO35
#NET "PIO<35>" LOC = "C14"; # Bank = 0, Pin name = IO_L03N_0/VREF_0, Type = VREF, Sch name = R-IO36
#NET "PIO<36>" LOC = "D14"; # Bank = 0, Pin name = IO_L03P_0, Type = I/O, Sch name = R-IO37
#NET "PIO<37>" LOC = "B14"; # Bank = 0, Pin name = IO_L04P_0, Type = I/O, Sch name = R-IO38
#NET "PIO<38>" LOC = "A16"; # Bank = 0, Pin name = IO_L01N_0, Type = I/O, Sch name = R-IO39
#NET "PIO<39>" LOC = "B16"; # Bank = 0, Pin name = IO_L01P_0, Type = I/O, Sch name = R-IO40
 
## 12 pin connectors
#NET "JA<0>" LOC = "L15"; # Bank = 1, Pin name = IO_L09N_1/A11, Type = DUAL, Sch name = JA1
#NET "JA<1>" LOC = "K12"; # Bank = 1, Pin name = IO_L11N_1/A9/RHCLK1, Type = RHCLK/DUAL, Sch name = JA2
#NET "JA<2>" LOC = "L17"; # Bank = 1, Pin name = IO_L10N_1/VREF_1, Type = VREF, Sch name = JA3
#NET "JA<3>" LOC = "M15"; # Bank = 1, Pin name = IO_L07P_1, Type = I/O, Sch name = JA4
#NET "JA<4>" LOC = "K13"; # Bank = 1, Pin name = IO_L11P_1/A10/RHCLK0, Type = RHCLK/DUAL, Sch name = JA7
#NET "JA<5>" LOC = "L16"; # Bank = 1, Pin name = IO_L09P_1/A12, Type = DUAL, Sch name = JA8
#NET "JA<6>" LOC = "M14"; # Bank = 1, Pin name = IO_L05P_1, Type = I/O, Sch name = JA9
#NET "JA<7>" LOC = "M16"; # Bank = 1, Pin name = IO_L07N_1, Type = I/O, Sch name = JA10
#NET "JB<0>" LOC = "M13"; # Bank = 1, Pin name = IO_L05N_1/VREF_1, Type = VREF, Sch name = JB1
#NET "JB<1>" LOC = "R18"; # Bank = 1, Pin name = IO_L02P_1/A14, Type = DUAL, Sch name = JB2
#NET "JB<2>" LOC = "R15"; # Bank = 1, Pin name = IO_L03P_1, Type = I/O, Sch name = JB3
#NET "JB<3>" LOC = "T17"; # Bank = 1, Pin name = IO_L01N_1/A15, Type = DUAL, Sch name = JB4
#NET "JB<4>" LOC = "P17"; # Bank = 1, Pin name = IO_L06P_1, Type = I/O, Sch name = JB7
#NET "JB<5>" LOC = "R16"; # Bank = 1, Pin name = IO_L03N_1/VREF_1, Type = VREF, Sch name = JB8
#NET "JB<6>" LOC = "T18"; # Bank = 1, Pin name = IO_L02N_1/A13, Type = DUAL, Sch name = JB9
#NET "JB<7>" LOC = "U18"; # Bank = 1, Pin name = IO_L01P_1/A16, Type = DUAL, Sch name = JB10
#NET "JC<0>" LOC = "G15"; # Bank = 1, Pin name = IO_L18P_1, Type = I/O, Sch name = JC1
#NET "JC<1>" LOC = "J16"; # Bank = 1, Pin name = IO_L13N_1/A5/RHCLK5, Type = RHCLK/DUAL, Sch name = JC2
#NET "JC<2>" LOC = "G13"; # Bank = 1, Pin name = IO_L20N_1, Type = I/O, Sch name = JC3
#NET "JC<3>" LOC = "H16"; # Bank = 1, Pin name = IO_L16P_1, Type = I/O, Sch name = JC4
#NET "JC<4>" LOC = "H15"; # Bank = 1, Pin name = IO_L17N_1, Type = I/O, Sch name = JC7
#NET "JC<5>" LOC = "F14"; # Bank = 1, Pin name = IO_L21N_1, Type = I/O, Sch name = JC8
#NET "JC<6>" LOC = "G16"; # Bank = 1, Pin name = IO_L18N_1, Type = I/O, Sch name = JC9
#NET "JC<7>" LOC = "J12"; # Bank = 1, Pin name = IO_L15P_1/A2, Type = DUAL, Sch name = JC10
#NET "JD<0>" LOC = "J13"; # Bank = 1, Pin name = IO_L15N_1/A1, Type = DUAL, Sch name = JD1
#NET "JD<1>" LOC = "M18"; # Bank = 1, Pin name = IO_L08N_1, Type = I/O, Sch name = JD2
#NET "JD<2>" LOC = "N18"; # Bank = 1, Pin name = IO_L08P_1, Type = I/O, Sch name = JD3
#NET "JD<3>" LOC = "P18"; # Bank = 1, Pin name = IO_L06N_1, Type = I/O, Sch name = JD4
 
## onBoard USB controller
#NET "EppAstb"   LOC = "V14"; # Bank = 2, Pin name = IP_L23P_2, Type = INPUT, Sch name = U-FLAGA
#NET "EppDstb"   LOC = "U14"; # Bank = 2, Pin name = IP_L23N_2, Type = INPUT, Sch name = U-FLAGB
#NET "UsbFlag"   LOC = "V16"; # Bank = 2, Pin name = IP, Type = INPUT, Sch name = U-FLAGC
#NET "EppWait"   LOC = "N9"; # Bank = 2, Pin name = IO_L12P_2/D7/GCLK12, Type = DUAL/GCLK, Sch name = U-SLRD
#NET "EppDB<0>"  LOC = "R14"; # Bank = 2, Pin name = IO_L24N_2/A20, Type = DUAL, Sch name = U-FD0
#NET "EppDB<1>"  LOC = "R13"; # Bank = 2, Pin name = IO_L22N_2/A22, Type = DUAL, Sch name = U-FD1
#NET "EppDB<2>"  LOC = "P13"; # Bank = 2, Pin name = IO_L22P_2/A23, Type = DUAL, Sch name = U-FD2
#NET "EppDB<3>"  LOC = "T12"; # Bank = 2, Pin name = IO_L20P_2, Type = I/O, Sch name = U-FD3
#NET "EppDB<4>"  LOC = "N11"; # Bank = 2, Pin name = IO_L18N_2, Type = I/O, Sch name = U-FD4
#NET "EppDB<5>"  LOC = "R11"; # Bank = 2, Pin name = IO, Type = I/O, Sch name = U-FD5
#NET "EppDB<6>"  LOC = "P10"; # Bank = 2, Pin name = IO_L15N_2/D1/GCLK3, Type = DUAL/GCLK, Sch name = U-FD6
#NET "EppDB<7>"  LOC = "R10"; # Bank = 2, Pin name = IO_L15P_2/D2/GCLK2, Type = DUAL/GCLK, Sch name = U-FD7
 
#NET "UsbClk" LOC = "T15"; # Bank = 2, Pin name = IO/VREF_2, Type = VREF, Sch name = U-IFCLK
 
#NET "UsbOE"     LOC = "V15"; # Bank = 2, Pin name = IO_L25P_2/VS2/A19, Type = DUAL, Sch name = U-SLOE
#NET "UsbWR"     LOC = "V9";  # Bank = 2, Pin name = IO_L13N_2/D3/GCLK15, Type = DUAL/GCLK, Sch name = U-SWLR
#NET "UsbPktEnd" LOC = "V12"; # Bank = 2, Pin name = IO_L19P_2, Type = I/O, Sch name = U-PKTEND
 
#NET "UsbDir"    LOC = "T16"; # Bank = 2, Pin name = IO_L26P_2/VS0/A17, Type = DUAL, Sch name = U-SLCS
#NET "UsbMode"   LOC = "U15"; # Bank = 2, Pin name = IO_L25N_2/VS1/A18, Type = DUAL, Sch name = U-INT0#
 
#NET "UsbAdr<0>" LOC = "T14"; # Bank = 2, Pin name = IO_L24P_2/A21, Type = DUAL, Sch name = U-FIFOAD0
#NET "UsbAdr<1>" LOC = "V13"; # Bank = 2, Pin name = IO_L19N_2/VREF_2, Type = VREF, Sch name = U-FIFOAD1
 
##NET "UsbRdy"   LOC = "U13"; # Bank = 2, Pin name = IP, Type = INPUT, Sch name = U-RDY
